
**** Log buffer [000001] 2018-11-30_02:25:45 ****

[  0.033] Opening device: \\.\COM3
[  0.039] Detecting device
[ 34.077] ERROR: sahara_greet_device()->change_mode()->do_hello()->IO error
[ 34.077] Check qboot_log.txt for more details
[ 34.079] Total time: 34.081s
[ 34.079] 
[ 34.079] qboot version 3.86
[ 34.079] 
[ 34.079] DEVICE {
[ 34.079]   name  = "\\.\COM3",
[ 34.079]   flags = "0x64",
[ 34.079]   addr  = "0x62FD54",
[ 34.079]   api.bnr = "0xEA2E18",
[ 34.079] }
[ 34.079] 
[ 34.079] 
[ 34.079] Backup & Restore {
[ 34.079]   num_entries = 0,
[ 34.079]   restoring = "false",
[ 34.079]   backup_error = "not started",
[ 34.079]   restore_error = "not started",
[ 34.079] }
[ 34.079] 

**** Log buffer [000001] 2018-11-30_02:27:02 ****

[ -0.000] Opening device: \\.\COM3
[  0.002] Detecting device
[ 34.077] ERROR: sahara_greet_device()->change_mode()->do_hello()->IO error
[ 34.077] Check qboot_log.txt for more details
[ 34.078] Total time: 34.079s
[ 34.078] 
[ 34.078] qboot version 3.86
[ 34.078] 
[ 34.078] DEVICE {
[ 34.078]   name  = "\\.\COM3",
[ 34.078]   flags = "0x64",
[ 34.078]   addr  = "0x62FD54",
[ 34.078]   api.bnr = "0xE42E18",
[ 34.078] }
[ 34.078] 
[ 34.078] 
[ 34.078] Backup & Restore {
[ 34.078]   num_entries = 0,
[ 34.078]   restoring = "false",
[ 34.078]   backup_error = "not started",
[ 34.078]   restore_error = "not started",
[ 34.078] }
[ 34.078] 

**** Log buffer [000001] 2018-11-30_02:28:00 ****

[ -0.000] Opening device: \\.\COM3
[  0.002] Detecting device
[ 34.038] ERROR: sahara_greet_device()->change_mode()->do_hello()->IO error
[ 34.038] Check qboot_log.txt for more details
[ 34.038] Total time: 34.039s
[ 34.038] 
[ 34.038] qboot version 3.86
[ 34.038] 
[ 34.038] DEVICE {
[ 34.038]   name  = "\\.\COM3",
[ 34.038]   flags = "0x64",
[ 34.038]   addr  = "0x62FD54",
[ 34.038]   api.bnr = "0xFA2E48",
[ 34.038] }
[ 34.038] 
[ 34.038] 
[ 34.038] Backup & Restore {
[ 34.038]   num_entries = 0,
[ 34.038]   restoring = "false",
[ 34.038]   backup_error = "not started",
[ 34.038]   restore_error = "not started",
[ 34.038] }
[ 34.038] 

**** Log buffer [000001] 2018-11-30_02:28:58 ****

[ -0.000] Opening device: \\.\COM3
[  0.002] Detecting device
[ 34.037] ERROR: sahara_greet_device()->change_mode()->do_hello()->IO error
[ 34.037] Check qboot_log.txt for more details
[ 34.037] Total time: 34.038s
[ 34.038] 
[ 34.038] qboot version 3.86
[ 34.038] 
[ 34.038] DEVICE {
[ 34.038]   name  = "\\.\COM3",
[ 34.038]   flags = "0x64",
[ 34.038]   addr  = "0x62FD54",
[ 34.038]   api.bnr = "0x10B2E48",
[ 34.038] }
[ 34.038] 
[ 34.038] 
[ 34.038] Backup & Restore {
[ 34.038]   num_entries = 0,
[ 34.038]   restoring = "false",
[ 34.038]   backup_error = "not started",
[ 34.038]   restore_error = "not started",
[ 34.038] }
[ 34.038] 

**** Log buffer [000001] 2018-11-30_02:29:41 ****

[  0.001] Opening device: \\.\COM3
[  0.002] Detecting device
[ 34.034] ERROR: sahara_greet_device()->change_mode()->do_hello()->IO error
[ 34.034] Check qboot_log.txt for more details
[ 34.035] Total time: 34.036s
[ 34.035] 
[ 34.035] qboot version 3.86
[ 34.035] 
[ 34.035] DEVICE {
[ 34.035]   name  = "\\.\COM3",
[ 34.035]   flags = "0x64",
[ 34.035]   addr  = "0x62FD54",
[ 34.035]   api.bnr = "0x782E48",
[ 34.035] }
[ 34.035] 
[ 34.035] 
[ 34.035] Backup & Restore {
[ 34.035]   num_entries = 0,
[ 34.035]   restoring = "false",
[ 34.035]   backup_error = "not started",
[ 34.035]   restore_error = "not started",
[ 34.035] }
[ 34.035] 

**** Log buffer [000001] 2018-11-30_02:30:59 ****

[ -0.000] Opening device: \\.\COM3
[  0.001] Detecting device
[ 34.042] ERROR: sahara_greet_device()->change_mode()->do_hello()->IO error
[ 34.042] Check qboot_log.txt for more details
[ 34.045] Total time: 34.047s
[ 34.048] 
[ 34.048] qboot version 3.86
[ 34.048] 
[ 34.048] DEVICE {
[ 34.048]   name  = "\\.\COM3",
[ 34.048]   flags = "0x64",
[ 34.048]   addr  = "0x62FD54",
[ 34.048]   api.bnr = "0x1002E48",
[ 34.048] }
[ 34.048] 
[ 34.048] 
[ 34.048] Backup & Restore {
[ 34.048]   num_entries = 0,
[ 34.048]   restoring = "false",
[ 34.048]   backup_error = "not started",
[ 34.048]   restore_error = "not started",
[ 34.048] }
[ 34.048] 

**** Log buffer [000001] 2018-11-30_02:34:11 ****

[ -0.000] Opening device: \\.\COM3
[  0.010] Detecting device
[ 34.043] ERROR: sahara_greet_device()->change_mode()->do_hello()->IO error
[ 34.043] Check qboot_log.txt for more details
[ 34.048] Total time: 34.048s
[ 34.048] 
[ 34.048] qboot version 3.86
[ 34.048] 
[ 34.048] DEVICE {
[ 34.048]   name  = "\\.\COM3",
[ 34.048]   flags = "0x64",
[ 34.048]   addr  = "0x62FD54",
[ 34.049]   api.bnr = "0xF42E48",
[ 34.049] }
[ 34.049] 
[ 34.049] 
[ 34.049] Backup & Restore {
[ 34.049]   num_entries = 0,
[ 34.049]   restoring = "false",
[ 34.049]   backup_error = "not started",
[ 34.049]   restore_error = "not started",
[ 34.050] }
[ 34.050] 

**** Log buffer [000001] 2018-11-30_02:36:21 ****

[  0.000] Opening device: \\.\COM3
[  0.002] Detecting device
[ 34.042] ERROR: sahara_greet_device()->change_mode()->do_hello()->IO error
[ 34.042] Check qboot_log.txt for more details
[ 34.047] Total time: 34.049s
[ 34.049] 
[ 34.049] qboot version 3.86
[ 34.049] 
[ 34.050] DEVICE {
[ 34.050]   name  = "\\.\COM3",
[ 34.050]   flags = "0x64",
[ 34.050]   addr  = "0x62FD54",
[ 34.050]   api.bnr = "0xF22E48",
[ 34.050] }
[ 34.050] 
[ 34.050] 
[ 34.050] Backup & Restore {
[ 34.050]   num_entries = 0,
[ 34.050]   restoring = "false",
[ 34.050]   backup_error = "not started",
[ 34.050]   restore_error = "not started",
[ 34.050] }
[ 34.050] 

**** Log buffer [000001] 2018-11-30_03:04:24 ****

[  0.000] Opening device: \\.\COM3
[  0.002] Detecting device
[  0.005] ...cpu.id  = 172 (0xac)
[  0.005] ...cpu.sn  = 4025254662 (0xefec8306)
[  0.005] Opening singleimage
[  0.005] Loading package
[  0.008] ...filename = pkg.xml
[  0.010] Loading programmer
[  0.011] ...filename = programmer.elf
[  0.011] Sending programmer
[  0.202] Handling things over to programmer
[  0.202] Identifying CPU version
[  0.202] Waiting for firehose to get ready
[  3.227] ...SDM630 1.0
[  3.227] Determining target secure state
[  3.230] ...secure = yes
[  3.267] Configuring device...
[  3.275] Flashing GPT...
[  3.275] Flashing partition with gpt.bin
[  3.279] Initializing storage
[  3.328] ...blksz = 512
[  3.490] Re-initializing storage...
[  3.490] Initializing storage
[  3.654] Flashing bootloader...
[  3.658] Flashing xbl_a with xbl.elf
[  4.002] WriteFile() failed, GetLastError()=0
[  4.012] ERROR: do_package()->do_recipe()->do_flash()->pt_write()->storage_write()->firehose_do_fmt()->do_recipe()->do_program()->send_raw()->IO error
[  4.034] Check qboot_log.txt for more details
[  4.040] Total time: 4.057s
[  4.042] 
[  4.042] qboot version 3.86
[  4.042] 
[  4.042] DEVICE {
[  4.042]   name  = "\\.\COM3",
[  4.042]   flags = "0x144",
[  4.042]   addr  = "0x62FD54",
[  4.042]   sahara.current_mode = "0",
[  4.042]   api.buffer = "0x2AC3020",
[  4.042]   cpu.serial = "4025254662",
[  4.042]   cpu.id = "172",
[  4.042]   cpu.sv_sbl = "1",
[  4.042]   cpu.name = "SDM630",
[  4.042]   storage.type = "eMMC",
[  4.042]   sahara.programmer = "programmer.elf",
[  4.042]   module.firehose = "0x6F1200",
[  4.042]   api.firehose = "0x1160D40",
[  4.042]   cpu.ver = "256",
[  4.042]   cpu.vername = "1.0",
[  4.042]   fh.max_packet_sz = "1048576",
[  4.042]   fh.storage_inited = "1",
[  4.042]   api.storage = "0x6F6308",
[  4.042]   api.bnr = "0x713390",
[  4.042] }
[  4.042] 
[  4.042] 
[  4.042] STORAGE {
[  4.042]   type = "eMMC",
[  4.042]   part  = "(null)",
[  4.042]   blksz = 512 (0x200),
[  4.042]   num_luns = 4,
[  4.042]   luns[00] = {
[  4.042]     size = 59640M,
[  4.042]     ptable[00] = { attrs.needs_bnr = 1, offset =     128K, size =    3584K, name = "xbl_a" },
[  4.042]     ptable[01] = { attrs.needs_bnr = 1, offset =    3712K, size =    3584K, name = "xbl_b" },
[  4.042]     ptable[02] = { attrs.needs_bnr = 1, offset =    7296K, size =       2M, name = "tz_a" },
[  4.042]     ptable[03] = { attrs.needs_bnr = 1, offset =    9344K, size =       2M, name = "tz_b" },
[  4.042]     ptable[04] = { attrs.needs_bnr = 1, offset =   11392K, size =     512K, name = "rpm_a" },
[  4.042]     ptable[05] = { attrs.needs_bnr = 1, offset =   11904K, size =     512K, name = "rpm_b" },
[  4.042]     ptable[06] = { attrs.needs_bnr = 1, offset =   12416K, size =     512K, name = "hyp_a" },
[  4.042]     ptable[07] = { attrs.needs_bnr = 1, offset =   12928K, size =     512K, name = "hyp_b" },
[  4.042]     ptable[08] = { attrs.needs_bnr = 1, offset =   13440K, size =     128K, name = "devcfg_a" },
[  4.042]     ptable[09] = { attrs.needs_bnr = 1, offset =   13568K, size =     128K, name = "devcfg_b" },
[  4.042]     ptable[10] = { attrs.needs_bnr = 1, offset =   13696K, size =     512K, name = "pmic_a" },
[  4.042]     ptable[11] = { attrs.needs_bnr = 1, offset =   14208K, size =     512K, name = "pmic_b" },
[  4.042]     ptable[12] = { attrs.needs_bnr = 1, offset =   14720K, size =       1M, name = "abl_a" },
[  4.042]     ptable[13] = { attrs.needs_bnr = 1, offset =   15744K, size =       1M, name = "abl_b" },
[  4.042]     ptable[14] = { attrs.needs_bnr = 1, offset =   16768K, size =     512K, name = "cmnlib_a" },
[  4.042]     ptable[15] = { attrs.needs_bnr = 1, offset =   17280K, size =     512K, name = "cmnlib64_a" },
[  4.042]     ptable[16] = { attrs.needs_bnr = 1, offset =   17792K, size =     512K, name = "cmnlib_b" },
[  4.042]     ptable[17] = { attrs.needs_bnr = 1, offset =   18304K, size =     512K, name = "cmnlib64_b" },
[  4.042]     ptable[18] = { attrs.needs_bnr = 1, offset =   18816K, size =     512K, name = "keymaster_a" },
[  4.042]     ptable[19] = { attrs.needs_bnr = 1, offset =   19328K, size =     512K, name = "keymaster_b" },
[  4.042]     ptable[20] = { attrs.needs_bnr = 1, offset =   19840K, size =     128K, name = "storsec_a" },
[  4.042]     ptable[21] = { attrs.needs_bnr = 1, offset =   19968K, size =     128K, name = "storsec_b" },
[  4.042]     ptable[22] = { attrs.needs_bnr = 1, offset =   20096K, size =     256K, name = "prov_a" },
[  4.042]     ptable[23] = { attrs.needs_bnr = 1, offset =   20352K, size =     256K, name = "prov_b" },
[  4.042]     ptable[24] = { attrs.needs_bnr = 0, offset =   20608K, size =     110M, name = "modem_a" },
[  4.042]     ptable[25] = { attrs.needs_bnr = 0, offset =  133248K, size =     110M, name = "modem_b" },
[  4.042]     ptable[26] = { attrs.needs_bnr = 0, offset =  245888K, size =       1K, name = "fsc" },
[  4.042]     ptable[27] = { attrs.needs_bnr = 0, offset =  245892K, size =       8K, name = "ssd" },
[  4.042]     ptable[28] = { attrs.needs_bnr = 0, offset =  246016K, size =      16M, name = "dsp_a" },
[  4.042]     ptable[29] = { attrs.needs_bnr = 0, offset =  262400K, size =      16M, name = "dsp_b" },
[  4.042]     ptable[30] = { attrs.needs_bnr = 0, offset =  278784K, size =       1M, name = "ddr" },
[  4.042]     ptable[31] = { attrs.needs_bnr = 1, offset =  279808K, size =     512K, name = "utags" },
[  4.042]     ptable[32] = { attrs.needs_bnr = 0, offset =  280320K, size =     512K, name = "utagsBackup" },
[  4.042]     ptable[33] = { attrs.needs_bnr = 0, offset =  280832K, size =       2M, name = "modemst1" },
[  4.042]     ptable[34] = { attrs.needs_bnr = 0, offset =  282880K, size =       2M, name = "modemst2" },
[  4.042]     ptable[35] = { attrs.needs_bnr = 0, offset =  284928K, size =       6M, name = "fsg_a" },
[  4.042]     ptable[36] = { attrs.needs_bnr = 0, offset =  291072K, size =       6M, name = "fsg_b" },
[  4.042]     ptable[37] = { attrs.needs_bnr = 1, offset =  297216K, size =      32M, name = "persist" },
[  4.042]     ptable[38] = { attrs.needs_bnr = 1, offset =  329984K, size =     512K, name = "frp" },
[  4.042]     ptable[39] = { attrs.needs_bnr = 1, offset =  330496K, size =     128K, name = "cid" },
[  4.042]     ptable[40] = { attrs.needs_bnr = 0, offset =  330624K, size =      16M, name = "carrier" },
[  4.042]     ptable[41] = { attrs.needs_bnr = 0, offset =  347008K, size =     512K, name = "metadata" },
[  4.042]     ptable[42] = { attrs.needs_bnr = 0, offset =  347520K, size =       8M, name = "kpan" },
[  4.042]     ptable[43] = { attrs.needs_bnr = 0, offset =  355712K, size =      64M, name = "boot_a" },
[  4.042]     ptable[44] = { attrs.needs_bnr = 0, offset =  421248K, size =      64M, name = "boot_b" },
[  4.042]     ptable[45] = { attrs.needs_bnr = 0, offset =  486784K, size =      16M, name = "dto_a" },
[  4.042]     ptable[46] = { attrs.needs_bnr = 0, offset =  503168K, size =      16M, name = "dto_b" },
[  4.042]     ptable[47] = { attrs.needs_bnr = 1, offset =  519552K, size =       1M, name = "misc" },
[  4.042]     ptable[48] = { attrs.needs_bnr = 0, offset =  520576K, size =       8M, name = "logfs" },
[  4.042]     ptable[49] = { attrs.needs_bnr = 0, offset =  528768K, size =     256K, name = "apdp" },
[  4.042]     ptable[50] = { attrs.needs_bnr = 0, offset =  529024K, size =     256K, name = "msadp" },
[  4.042]     ptable[51] = { attrs.needs_bnr = 0, offset =  529280K, size =       1K, name = "dpo" },
[  4.042]     ptable[52] = { attrs.needs_bnr = 1, offset =  529284K, size =       1K, name = "devinfo" },
[  4.042]     ptable[53] = { attrs.needs_bnr = 0, offset =  529288K, size =    4608K, name = "bluetooth_a" },
[  4.042]     ptable[54] = { attrs.needs_bnr = 0, offset =  533896K, size =    4608K, name = "bluetooth_b" },
[  4.042]     ptable[55] = { attrs.needs_bnr = 0, offset =  538504K, size =   33424K, name = "logo_a" },
[  4.042]     ptable[56] = { attrs.needs_bnr = 0, offset =  571928K, size =   33424K, name = "logo_b" },
[  4.042]     ptable[57] = { attrs.needs_bnr = 0, offset =  605352K, size =      64K, name = "vbmeta_a" },
[  4.042]     ptable[58] = { attrs.needs_bnr = 0, offset =  605416K, size =      64K, name = "vbmeta_b" },
[  4.042]     ptable[59] = { attrs.needs_bnr = 0, offset =  605480K, size =   17112K, name = "padA" },
[  4.042]     ptable[60] = { attrs.needs_bnr = 1, offset =     608M, size =       8M, name = "hw" },
[  4.042]     ptable[61] = { attrs.needs_bnr = 0, offset =     616M, size =       8M, name = "sp" },
[  4.042]     ptable[62] = { attrs.needs_bnr = 0, offset =     624M, size =     576M, name = "oem_a" },
[  4.042]     ptable[63] = { attrs.needs_bnr = 0, offset =    1200M, size =     576M, name = "oem_b" },
[  4.042]     ptable[64] = { attrs.needs_bnr = 0, offset =    1776M, size =    4128M, name = "system_a" },
[  4.042]     ptable[65] = { attrs.needs_bnr = 0, offset =    5904M, size =    4128M, name = "system_b" },
[  4.042]     ptable[66] = { attrs.needs_bnr = 0, offset =   10032M, size = 52017741312, name = "userdata" },
[  4.042]   }
[  4.042]   luns[01] = {
[  4.042]     size = 4M,
[  4.042]   }
[  4.042]   luns[02] = {
[  4.042]     size = 4M,
[  4.042]   }
[  4.042]   luns[03] = {
[  4.042]     size = 4M,
[  4.042]   }
[  4.042] }
[  4.042] 
[  4.042] 
[  4.042] Backup & Restore {
[  4.042]   num_entries = 0,
[  4.042]   restoring = "false",
[  4.042]   backup_error = "not started",
[  4.042]   restore_error = "not started",
[  4.042] }
[  4.042] 

**** Log buffer [000001] 2018-11-30_03:04:35 ****

[  0.000] Opening device: \\.\COM3
[  0.002] Detecting device
[  0.005] ...cpu.id  = 172 (0xac)
[  0.005] ...cpu.sn  = 4025254662 (0xefec8306)
[  0.005] Opening singleimage
[  0.006] Loading package
[  0.008] ...filename = pkg.xml
[  0.011] Loading programmer
[  0.011] ...filename = programmer.elf
[  0.012] Sending programmer
[  0.203] Handling things over to programmer
[  0.203] Identifying CPU version
[  0.203] Waiting for firehose to get ready
[  3.238] ...SDM630 1.0
[  3.239] Determining target secure state
[  3.242] ...secure = yes
[  3.283] Configuring device...
[  3.290] Flashing GPT...
[  3.290] Flashing partition with gpt.bin
[  3.295] Initializing storage
[  3.342] ...blksz = 512
[  3.508] Re-initializing storage...
[  3.509] Initializing storage
[  3.689] Flashing bootloader...
[  3.692] Flashing xbl_a with xbl.elf
[  4.078] WriteFile() failed, GetLastError()=0
[  4.082] ERROR: do_package()->do_recipe()->do_flash()->pt_write()->storage_write()->firehose_do_fmt()->do_recipe()->do_program()->send_raw()->IO error
[  4.091] Check qboot_log.txt for more details
[  4.093] Total time: 4.094s
[  4.096] 
[  4.096] qboot version 3.86
[  4.096] 
[  4.096] DEVICE {
[  4.096]   name  = "\\.\COM3",
[  4.096]   flags = "0x144",
[  4.096]   addr  = "0x62FD54",
[  4.096]   sahara.current_mode = "0",
[  4.096]   api.buffer = "0x2A9D020",
[  4.096]   cpu.serial = "4025254662",
[  4.096]   cpu.id = "172",
[  4.096]   cpu.sv_sbl = "1",
[  4.096]   cpu.name = "SDM630",
[  4.096]   storage.type = "eMMC",
[  4.096]   sahara.programmer = "programmer.elf",
[  4.096]   module.firehose = "0x29D1240",
[  4.096]   api.firehose = "0x1030D40",
[  4.096]   cpu.ver = "256",
[  4.096]   cpu.vername = "1.0",
[  4.096]   fh.max_packet_sz = "1048576",
[  4.096]   fh.storage_inited = "1",
[  4.096]   api.storage = "0x103D1A8",
[  4.096]   api.bnr = "0x29EC420",
[  4.096] }
[  4.096] 
[  4.096] 
[  4.096] STORAGE {
[  4.096]   type = "eMMC",
[  4.096]   part  = "(null)",
[  4.096]   blksz = 512 (0x200),
[  4.096]   num_luns = 4,
[  4.096]   luns[00] = {
[  4.096]     size = 59640M,
[  4.096]     ptable[00] = { attrs.needs_bnr = 1, offset =     128K, size =    3584K, name = "xbl_a" },
[  4.096]     ptable[01] = { attrs.needs_bnr = 1, offset =    3712K, size =    3584K, name = "xbl_b" },
[  4.096]     ptable[02] = { attrs.needs_bnr = 1, offset =    7296K, size =       2M, name = "tz_a" },
[  4.096]     ptable[03] = { attrs.needs_bnr = 1, offset =    9344K, size =       2M, name = "tz_b" },
[  4.096]     ptable[04] = { attrs.needs_bnr = 1, offset =   11392K, size =     512K, name = "rpm_a" },
[  4.096]     ptable[05] = { attrs.needs_bnr = 1, offset =   11904K, size =     512K, name = "rpm_b" },
[  4.096]     ptable[06] = { attrs.needs_bnr = 1, offset =   12416K, size =     512K, name = "hyp_a" },
[  4.096]     ptable[07] = { attrs.needs_bnr = 1, offset =   12928K, size =     512K, name = "hyp_b" },
[  4.096]     ptable[08] = { attrs.needs_bnr = 1, offset =   13440K, size =     128K, name = "devcfg_a" },
[  4.096]     ptable[09] = { attrs.needs_bnr = 1, offset =   13568K, size =     128K, name = "devcfg_b" },
[  4.096]     ptable[10] = { attrs.needs_bnr = 1, offset =   13696K, size =     512K, name = "pmic_a" },
[  4.096]     ptable[11] = { attrs.needs_bnr = 1, offset =   14208K, size =     512K, name = "pmic_b" },
[  4.096]     ptable[12] = { attrs.needs_bnr = 1, offset =   14720K, size =       1M, name = "abl_a" },
[  4.096]     ptable[13] = { attrs.needs_bnr = 1, offset =   15744K, size =       1M, name = "abl_b" },
[  4.096]     ptable[14] = { attrs.needs_bnr = 1, offset =   16768K, size =     512K, name = "cmnlib_a" },
[  4.096]     ptable[15] = { attrs.needs_bnr = 1, offset =   17280K, size =     512K, name = "cmnlib64_a" },
[  4.096]     ptable[16] = { attrs.needs_bnr = 1, offset =   17792K, size =     512K, name = "cmnlib_b" },
[  4.096]     ptable[17] = { attrs.needs_bnr = 1, offset =   18304K, size =     512K, name = "cmnlib64_b" },
[  4.096]     ptable[18] = { attrs.needs_bnr = 1, offset =   18816K, size =     512K, name = "keymaster_a" },
[  4.096]     ptable[19] = { attrs.needs_bnr = 1, offset =   19328K, size =     512K, name = "keymaster_b" },
[  4.096]     ptable[20] = { attrs.needs_bnr = 1, offset =   19840K, size =     128K, name = "storsec_a" },
[  4.096]     ptable[21] = { attrs.needs_bnr = 1, offset =   19968K, size =     128K, name = "storsec_b" },
[  4.096]     ptable[22] = { attrs.needs_bnr = 1, offset =   20096K, size =     256K, name = "prov_a" },
[  4.096]     ptable[23] = { attrs.needs_bnr = 1, offset =   20352K, size =     256K, name = "prov_b" },
[  4.096]     ptable[24] = { attrs.needs_bnr = 0, offset =   20608K, size =     110M, name = "modem_a" },
[  4.096]     ptable[25] = { attrs.needs_bnr = 0, offset =  133248K, size =     110M, name = "modem_b" },
[  4.096]     ptable[26] = { attrs.needs_bnr = 0, offset =  245888K, size =       1K, name = "fsc" },
[  4.096]     ptable[27] = { attrs.needs_bnr = 0, offset =  245892K, size =       8K, name = "ssd" },
[  4.096]     ptable[28] = { attrs.needs_bnr = 0, offset =  246016K, size =      16M, name = "dsp_a" },
[  4.096]     ptable[29] = { attrs.needs_bnr = 0, offset =  262400K, size =      16M, name = "dsp_b" },
[  4.096]     ptable[30] = { attrs.needs_bnr = 0, offset =  278784K, size =       1M, name = "ddr" },
[  4.096]     ptable[31] = { attrs.needs_bnr = 1, offset =  279808K, size =     512K, name = "utags" },
[  4.096]     ptable[32] = { attrs.needs_bnr = 0, offset =  280320K, size =     512K, name = "utagsBackup" },
[  4.096]     ptable[33] = { attrs.needs_bnr = 0, offset =  280832K, size =       2M, name = "modemst1" },
[  4.096]     ptable[34] = { attrs.needs_bnr = 0, offset =  282880K, size =       2M, name = "modemst2" },
[  4.096]     ptable[35] = { attrs.needs_bnr = 0, offset =  284928K, size =       6M, name = "fsg_a" },
[  4.096]     ptable[36] = { attrs.needs_bnr = 0, offset =  291072K, size =       6M, name = "fsg_b" },
[  4.096]     ptable[37] = { attrs.needs_bnr = 1, offset =  297216K, size =      32M, name = "persist" },
[  4.096]     ptable[38] = { attrs.needs_bnr = 1, offset =  329984K, size =     512K, name = "frp" },
[  4.096]     ptable[39] = { attrs.needs_bnr = 1, offset =  330496K, size =     128K, name = "cid" },
[  4.096]     ptable[40] = { attrs.needs_bnr = 0, offset =  330624K, size =      16M, name = "carrier" },
[  4.096]     ptable[41] = { attrs.needs_bnr = 0, offset =  347008K, size =     512K, name = "metadata" },
[  4.096]     ptable[42] = { attrs.needs_bnr = 0, offset =  347520K, size =       8M, name = "kpan" },
[  4.096]     ptable[43] = { attrs.needs_bnr = 0, offset =  355712K, size =      64M, name = "boot_a" },
[  4.096]     ptable[44] = { attrs.needs_bnr = 0, offset =  421248K, size =      64M, name = "boot_b" },
[  4.096]     ptable[45] = { attrs.needs_bnr = 0, offset =  486784K, size =      16M, name = "dto_a" },
[  4.096]     ptable[46] = { attrs.needs_bnr = 0, offset =  503168K, size =      16M, name = "dto_b" },
[  4.096]     ptable[47] = { attrs.needs_bnr = 1, offset =  519552K, size =       1M, name = "misc" },
[  4.096]     ptable[48] = { attrs.needs_bnr = 0, offset =  520576K, size =       8M, name = "logfs" },
[  4.096]     ptable[49] = { attrs.needs_bnr = 0, offset =  528768K, size =     256K, name = "apdp" },
[  4.096]     ptable[50] = { attrs.needs_bnr = 0, offset =  529024K, size =     256K, name = "msadp" },
[  4.096]     ptable[51] = { attrs.needs_bnr = 0, offset =  529280K, size =       1K, name = "dpo" },
[  4.097]     ptable[52] = { attrs.needs_bnr = 1, offset =  529284K, size =       1K, name = "devinfo" },
[  4.097]     ptable[53] = { attrs.needs_bnr = 0, offset =  529288K, size =    4608K, name = "bluetooth_a" },
[  4.097]     ptable[54] = { attrs.needs_bnr = 0, offset =  533896K, size =    4608K, name = "bluetooth_b" },
[  4.097]     ptable[55] = { attrs.needs_bnr = 0, offset =  538504K, size =   33424K, name = "logo_a" },
[  4.097]     ptable[56] = { attrs.needs_bnr = 0, offset =  571928K, size =   33424K, name = "logo_b" },
[  4.097]     ptable[57] = { attrs.needs_bnr = 0, offset =  605352K, size =      64K, name = "vbmeta_a" },
[  4.097]     ptable[58] = { attrs.needs_bnr = 0, offset =  605416K, size =      64K, name = "vbmeta_b" },
[  4.097]     ptable[59] = { attrs.needs_bnr = 0, offset =  605480K, size =   17112K, name = "padA" },
[  4.097]     ptable[60] = { attrs.needs_bnr = 1, offset =     608M, size =       8M, name = "hw" },
[  4.097]     ptable[61] = { attrs.needs_bnr = 0, offset =     616M, size =       8M, name = "sp" },
[  4.097]     ptable[62] = { attrs.needs_bnr = 0, offset =     624M, size =     576M, name = "oem_a" },
[  4.097]     ptable[63] = { attrs.needs_bnr = 0, offset =    1200M, size =     576M, name = "oem_b" },
[  4.097]     ptable[64] = { attrs.needs_bnr = 0, offset =    1776M, size =    4128M, name = "system_a" },
[  4.097]     ptable[65] = { attrs.needs_bnr = 0, offset =    5904M, size =    4128M, name = "system_b" },
[  4.097]     ptable[66] = { attrs.needs_bnr = 0, offset =   10032M, size = 52017741312, name = "userdata" },
[  4.097]   }
[  4.097]   luns[01] = {
[  4.097]     size = 4M,
[  4.097]   }
[  4.097]   luns[02] = {
[  4.097]     size = 4M,
[  4.097]   }
[  4.097]   luns[03] = {
[  4.097]     size = 4M,
[  4.097]   }
[  4.097] }
[  4.097] 
[  4.097] 
[  4.097] Backup & Restore {
[  4.097]   num_entries = 0,
[  4.097]   restoring = "false",
[  4.097]   backup_error = "not started",
[  4.097]   restore_error = "not started",
[  4.097] }
[  4.097] 
